{"text_format":"1","workbook":"xlsx","n_sheets":2,"sheets":["COMMAND PAGE","DATA PAGE"],"not_rendered":{"charts":0,"images":2,"macros":1,"external_links":0,"defined_names":6,"comments":1,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"COMMAND PAGE","index":0,"n_rows":46,"n_cols":8,"rows_kept":46,"cut":false,"hidden":false,"merged":[[9,4,9,11],[13,4,13,11],[14,4,14,11],[15,4,15,11],[10,4,12,11],[5,1,5,2],[0,1,1,2],[8,1,8,2],[0,4,0,11],[1,4,1,11],[4,4,5,11],[2,4,2,11],[3,4,3,11],[7,4,8,11],[18,5,20,11],[16,4,16,11],[46,4,46,11],[32,4,34,11],[30,5,30,11],[21,4,21,11],[36,7,40,10],[26,4,26,11],[27,5,28,11],[22,5,25,11],[29,4,29,11],[31,4,31,11],[44,4,44,11],[45,4,45,11],[42,4,43,11],[17,4,17,11]]}
[null,"Settings",null,null,"Instructions"]
[]
[null,"Comm Port",1,null,"See the RDP manual for the 650 or E725 for the commands required to get data back from the units. "]
[null,"Baud Rate",9600]
[null,"Time Out (Seconds)",1,null,"For a 650 unit the command #nn SCAN will cause the data from all enabled channels to be transmitted in ascending order of their channel address."]
[]
[null,"Number of Repeats","M"]
[null,"Data Direction","ACROSS",null,"For an E725, #nn SCAN will cause the data from the currently selected channel to be transmitted. Note, some older E725 units require the command #nn PRINT DATA to be sent."]
[]
[null,"Update Screen Whilst Logging","YES"]
[null,null,null,null,"Enter the commands you wish to send to the serial device(s) in the column below 'Commands'. They will be sent exactly as they are typed. All commands should be entered in the correct format for the receiving device, with the device address. Please note, that if not entered in the cell, a hash (#) will be added to the start of all transmissions. "]
[]
[]
[]
[null,null,null,null,"E.g., to get all the data from enable channels of the 650 at address 01, type '#01 SCAN'"]
[null,"COMMANDS"]
[null,null,null,null,"Other instructions are:-"]
[]
[null,null,null,null,"WAIT XXX. ","This causes the macro to wait for the specified number of SECONDS. Ensure that there is a space between the command and the time value and no other spaces. Decimal values of seconds are allowed.  E.g., WAIT 0.25 causes an approximate delay of 250ms. THIS TIMER IS NOT CALIBRATED."]
[]
[]
[]
[null,null,null,null,"RETURN.","The point on the Data Page where the data is written is reset. That is if data is being written across, the next piece of data will be written from the left margin of the data area, in the next row down. Conversely, if the data is being written down, subsequent data will be written from the top of the spreadsheet, in the next column."]
[]
[]
[]
[]
[null,null,null,null,"TIME. ","Inserts the current time and date in the current cell and then moves the data cell pointer on cell in the direction indicated in 'Data Direction'. The time is obtained from the PC clock."]
[]
[]
[null,null,null,null,"UPDATE","If screen updating is turned off, this command will cause the data page to be refreshed once."]
[]
[null,null,null,null,"Full example:- To log all enabled channels on 650/725 modules 01 and 02, inserting the time at the start of each row, starting a new row after each command loop and waiting 2 seconds between each loop the following command sequence would be necessary."]
[]
[]
[]
[null,null,null,null,null,"TIME","Disclaimer","This spreadsheet and the associated macro are supplied on a shareware basis. RDP offer no warranty or support for this software and accept no responsibility for errors or omissions. The software is used entirely at the user's risk."]
[null,null,null,null,null,"#01 SCAN"]
[null,null,null,null,null,"#02 SCAN"]
[null,null,null,null,null,"RETURN"]
[null,null,null,null,null,"WAIT 2"]
[]
[null,null,null,null,"RDP Electronics Limited"]
[]
[null,null,null,null,"Home Pages : www.rdpe.com"]
[null,null,null,null,"E-Mail : sales@rdpe.com"]

{"sheet":"DATA PAGE","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}